-->

## /*****************************************PORT HW-SW MAP*****************************************/

Table 1: PORT SFR Usage per API
API Name | SFRs Used | Remarks
--- | --- | ---
Port_Init | Pn_PDR,Pn_OUT,Pn_IOCR,Pn_DISC, Pn_LPCR,Pn_PCSR,Pn_OMR | n refers to port number | -
Port_RefreshPortDirection | Pn_IOCR | n refers to port number
Port_SetPinMode | Pn_IOCR | n refers to port number

## /******************************************PORT MPU Settings******************************************/

Table 2: PORT SFR and Memory Range
Start Address | End Address | Remarks
--- | --- | ---
PORT_START_SEC_VAR_32BIT | PORT_STOP_SEC_VAR_32BIT | Port_kConfigPtr - 32 bit variable used by PORT
PORT_START_SEC_CODE | PORT_STOP_SEC_CODE | PORT driver - Basic AUTOSAR and SAFETY functionality
PORT_START_SEC_CONST_16BIT | PORT_STOP_SEC_CONST_16BIT | Port_kAvailablePins - 16 bit constant used by PORT